Price 4000 ( 2 pieces 7000)

**Description**:

Electric Hot Water Heater Faucet 3000W Instant Heating Faucet 360 Degree Rotation Tankless Water Heater Temperature Adjustable Digital Kitchen Bathroom Supplies  
**Feature:**  
**1. Energy-Efficient Design:** Reduce energy consumption by 30% with a water-saving outlet, saving both electricity and water. The hot water heater faucet is designed with a water-saving outlet, greatly reducing water usage while maintaining optimal performance. It consumes 30% less energy compared to traditional models, resulting in cost savings and environmental benefits.  
**2. Versatile and Adjustable:**Equipped with a flexible hose that rotates freely, increasing usability and compatibility in kitchen and bathroom settings. The swivel hose of  kitchen instant heating faucet allows for easy maneuvering, providing greater flexibility and convenience during use. Suitable for various environments, such as kitchens and bathrooms, with adjustable temperature settings to meet different user preferences.  
**3. Smart Instant Heating:** Enjoy hot water within 3 seconds thanks to the intelligent rapid-heating faucet. The faucet utilizes advanced technology to heat water instantly, reducing waiting time and providing immediate hot water whenever needed. The smart digital display enables precise temperature control, ensuring a comfortable and customized water experience.  
**4. Water Pressure Considerations:**Please note that the hot cold mixer tap requires a certain water pressure to function properly, and it is not recommended for users with low water pressure or unconventional water sources. The product's functionality depends on adequate water pressure, so customers relying on non-municipal water sources or having water pressure lower than 6 meters may find this product unsuitable. For optimum performance and longevity, it is important to ensure the water pressure meets the product's requirements.  
**5. Installation Guidelines:** Prior to installation, please follow specific instructions to ensure proper setup and avoid potential issues. Confirm the water inlet method before purchasing to ensure compatibility with your current plumbing system, preventing installation complications. Installation should be done in an upward position only, strictly avoiding sideways, flat, or inverted installations for safety and optimal performance.

**Specification:**  
Certification: NONE  
Origin: Mainland China  
Number of Handles: Single Handle  
Valve Core Material: Brass  
Number of Holes for Installation: 2 Holes  
Spray Type: Side  
Rotatable Or Not: Yes  
Model Number: Tankless Instant Water Heater   
Feature: Thermostatic Faucets,Electric Faucets,Cold and Hot  
Style: Contemporary  
Type: Steel Ball Spool  
Style: Single Holder Single Hole  
Cold & Hot Water: Yes  
Material: Brass  
Dimensions: 290x230 mm /11.42x9.06 inches  
Material: ABS+stainless steel pipe  
Stainless steel pipe diameter: 4 points  
Hot water temperature: 30-60 degrees Celsius  
Waterproof grade: IPX4  
Rated pressure: 0.15-0.6MPa  
Power cord length: 1.1m  
Rated power: 3000W  
Specifications: 110V US regulation bottom water inlet / 220V European regulation bottom water inlet / 110V US regulation side water inlet / 220V European regulation side water inlet (optional)  
A : Bottom water inlet B: Side water inlet

**Note:**  
Due to the different monitor and light effect, the actual color of the item might be slightly different from the color showed on the pictures. Thank you!  
Please allow 1-2cm measuring deviation due to manual measurement.